ICU 75.1 75.1

Data Structures | Namespaces | Macros | Enumerations | Functions
ucptrie.h File Reference

C API: This file defines an immutable Unicode code point trie. More...

`#include "unicode/utypes.h"`
`#include "unicode/ucpmap.h"`
`#include "unicode/utf8.h"`
`#include "unicode/localpointer.h"`

Go to the source code of this file.

## Data Structures
struct | UCPTrie
| Immutable Unicode code point trie structure. More...

## Namespaces
| icu
| File coll.h.

## Macros
#define | UCPTRIE_16(trie, i) ((trie)->data.ptr16[i])
| Macro parameter value for a trie with 16-bit data values. More...
#define | UCPTRIE_32(trie, i) ((trie)->data.ptr32[i])
| Macro parameter value for a trie with 32-bit data values. More...
#define | UCPTRIE_8(trie, i) ((trie)->data.ptr8[i])
| Macro parameter value for a trie with 8-bit data values. More...
#define | UCPTRIE_FAST_GET(trie, dataAccess, c) dataAccess(trie, _UCPTRIE_CP_INDEX(trie, 0xffff, c))
| Returns a trie value for a code point, with range checking. More...
#define | UCPTRIE_SMALL_GET(trie, dataAccess, c) dataAccess(trie, _UCPTRIE_CP_INDEX(trie, UCPTRIE_SMALL_MAX, c))
| Returns a 16-bit trie value for a code point, with range checking. More...
#define | UCPTRIE_FAST_U16_NEXT(trie, dataAccess, src, limit, c, result)
| UTF-16: Reads the next code point (UChar32 c, out), post-increments src, and gets a value from the trie. More...
#define | UCPTRIE_FAST_U16_PREV(trie, dataAccess, start, src, c, result)
| UTF-16: Reads the previous code point (UChar32 c, out), pre-decrements src, and gets a value from the trie. More...
#define | UCPTRIE_FAST_U8_NEXT(trie, dataAccess, src, limit, result)
| UTF-8: Post-increments src and gets a value from the trie. More...
#define | UCPTRIE_FAST_U8_PREV(trie, dataAccess, start, src, result)
| UTF-8: Pre-decrements src and gets a value from the trie. More...
#define | UCPTRIE_ASCII_GET(trie, dataAccess, c) dataAccess(trie, c)
| Returns a trie value for an ASCII code point, without range checking. More...
#define | UCPTRIE_FAST_BMP_GET(trie, dataAccess, c) dataAccess(trie, _UCPTRIE_FAST_INDEX(trie, c))
| Returns a trie value for a BMP code point (U+0000..U+FFFF), without range checking. More...
#define | UCPTRIE_FAST_SUPP_GET(trie, dataAccess, c) dataAccess(trie, _UCPTRIE_SMALL_INDEX(trie, c))
| Returns a trie value for a supplementary code point (U+10000..U+10FFFF), without range checking. More...

## Enumerations
enum | UCPTrieType { UCPTRIE_TYPE_ANY = -1 , UCPTRIE_TYPE_FAST , UCPTRIE_TYPE_SMALL }
| Selectors for the type of a UCPTrie. More...
enum | UCPTrieValueWidth { UCPTRIE_VALUE_BITS_ANY = -1 , UCPTRIE_VALUE_BITS_16 , UCPTRIE_VALUE_BITS_32 , UCPTRIE_VALUE_BITS_8 }
| Selectors for the number of bits in a UCPTrie data value. More...

## Functions
U_CAPI UCPTrie * | ucptrie_openFromBinary (UCPTrieType type, UCPTrieValueWidth valueWidth, const void *data, int32_t length, int32_t *pActualLength, UErrorCode *pErrorCode)
| Opens a trie from its binary form, stored in 32-bit-aligned memory. More...
U_CAPI void | ucptrie_close (UCPTrie *trie)
| Closes a trie and releases associated memory. More...
U_CAPI UCPTrieType | ucptrie_getType (const UCPTrie *trie)
| Returns the trie type. More...
U_CAPI UCPTrieValueWidth | ucptrie_getValueWidth (const UCPTrie *trie)
| Returns the number of bits in a trie data value. More...
U_CAPI uint32_t | ucptrie_get (const UCPTrie *trie, UChar32 c)
| Returns the value for a code point as stored in the trie, with range checking. More...
U_CAPI UChar32 | ucptrie_getRange (const UCPTrie *trie, UChar32 start, UCPMapRangeOption option, uint32_t surrogateValue, UCPMapValueFilter *filter, const void *context, uint32_t *pValue)
| Returns the last code point such that all those from start to there have the same value. More...
U_CAPI int32_t | ucptrie_toBinary (const UCPTrie *trie, void *data, int32_t capacity, UErrorCode *pErrorCode)
| Writes a memory-mappable form of the trie into 32-bit aligned memory. More...

## Detailed Description

C API: This file defines an immutable Unicode code point trie.

See also
  UCPTrie
  UMutableCPTrie

Definition in file ucptrie.h.

## Macro Definition Documentation

## ◆ UCPTRIE_16

#define UCPTRIE_16 | ( |  | trie,
|  |  | i
| ) |  | ((trie)->data.ptr16[i])

Macro parameter value for a trie with 16-bit data values.

Use the name of this macro as a "dataAccess" parameter in other macros. Do not use this macro in any other way.

See also
  UCPTRIE_VALUE_BITS_16

Stable:
  ICU 63

Definition at line 326 of file ucptrie.h.

## ◆ UCPTRIE_32

#define UCPTRIE_32 | ( |  | trie,
|  |  | i
| ) |  | ((trie)->data.ptr32[i])

Macro parameter value for a trie with 32-bit data values.

Use the name of this macro as a "dataAccess" parameter in other macros. Do not use this macro in any other way.

See also
  UCPTRIE_VALUE_BITS_32

Stable:
  ICU 63

Definition at line 336 of file ucptrie.h.

## ◆ UCPTRIE_8

#define UCPTRIE_8 | ( |  | trie,
|  |  | i
| ) |  | ((trie)->data.ptr8[i])

Macro parameter value for a trie with 8-bit data values.

Use the name of this macro as a "dataAccess" parameter in other macros. Do not use this macro in any other way.

See also
  UCPTRIE_VALUE_BITS_8

Stable:
  ICU 63

Definition at line 346 of file ucptrie.h.

## ◆ UCPTRIE_ASCII_GET

#define UCPTRIE_ASCII_GET | ( |  | trie,
|  |  | dataAccess,
|  |  | c
| ) |  | dataAccess(trie, c)

Returns a trie value for an ASCII code point, without range checking.

Parameters

  trie | (const UCPTrie *, in) the trie (of either fast or small type)
  dataAccess | UCPTRIE_16, UCPTRIE_32, or UCPTRIE_8 according to the trie’s value width
  c | (UChar32, in) the input code point; must be U+0000..U+007F

Returns
  The ASCII code point's trie value.

Stable:
  ICU 63

Definition at line 517 of file ucptrie.h.

## ◆ UCPTRIE_FAST_BMP_GET

#define UCPTRIE_FAST_BMP_GET | ( |  | trie,
|  |  | dataAccess,
|  |  | c
| ) |  | dataAccess(trie, _UCPTRIE_FAST_INDEX(trie, c))

Returns a trie value for a BMP code point (U+0000..U+FFFF), without range checking.

Can be used to look up a value for a UTF-16 code unit if other parts of the string processing check for surrogates.

Parameters

  trie | (const UCPTrie *, in) the trie; must have type UCPTRIE_TYPE_FAST
  dataAccess | UCPTRIE_16, UCPTRIE_32, or UCPTRIE_8 according to the trie’s value width
  c | (UChar32, in) the input code point, must be U+0000..U+FFFF

Returns
  The BMP code point's trie value.

Stable:
  ICU 63

Definition at line 530 of file ucptrie.h.

## ◆ UCPTRIE_FAST_GET

#define UCPTRIE_FAST_GET | ( |  | trie,
|  |  | dataAccess,
|  |  | c
| ) |  | dataAccess(trie, _UCPTRIE_CP_INDEX(trie, 0xffff, c))

Returns a trie value for a code point, with range checking.

Returns the trie error value if c is not in the range 0..U+10FFFF.

Parameters

  trie | (const UCPTrie *, in) the trie; must have type UCPTRIE_TYPE_FAST
  dataAccess | UCPTRIE_16, UCPTRIE_32, or UCPTRIE_8 according to the trie’s value width
  c | (UChar32, in) the input code point

Returns
  The code point's trie value.

Stable:
  ICU 63

Definition at line 358 of file ucptrie.h.

## ◆ UCPTRIE_FAST_SUPP_GET

#define UCPTRIE_FAST_SUPP_GET | ( |  | trie,
|  |  | dataAccess,
|  |  | c
| ) |  | dataAccess(trie, _UCPTRIE_SMALL_INDEX(trie, c))

Returns a trie value for a supplementary code point (U+10000..U+10FFFF), without range checking.

Parameters

  trie | (const UCPTrie *, in) the trie; must have type UCPTRIE_TYPE_FAST
  dataAccess | UCPTRIE_16, UCPTRIE_32, or UCPTRIE_8 according to the trie’s value width
  c | (UChar32, in) the input code point, must be U+10000..U+10FFFF

Returns
  The supplementary code point's trie value.

Stable:
  ICU 63

Definition at line 542 of file ucptrie.h.

## ◆ UCPTRIE_FAST_U16_NEXT

#define UCPTRIE_FAST_U16_NEXT | ( |  | trie,
|  |  | dataAccess,
|  |  | src,
|  |  | limit,
|  |  | c,
|  |  | result
| ) |  |

Value:
UPRV_BLOCK_MACRO_BEGIN { \
(c) = *(src)++; \
int32_t __index; \
if (!U16_IS_SURROGATE(c)) { \
__index = _UCPTRIE_FAST_INDEX(trie, c); \
} else { \
uint16_t __c2; \
if (U16_IS_SURROGATE_LEAD(c) && (src) != (limit) && U16_IS_TRAIL(__c2 = *(src))) { \
++(src); \
(c) = U16_GET_SUPPLEMENTARY((c), __c2); \
__index = _UCPTRIE_SMALL_INDEX(trie, c); \
} else { \
__index = (trie)->dataLength - UCPTRIE_ERROR_VALUE_NEG_DATA_OFFSET; \
} \
} \
(result) = dataAccess(trie, __index); \
} UPRV_BLOCK_MACRO_END
UPRV_BLOCK_MACRO_END
#define UPRV_BLOCK_MACRO_END
Defined as "while (false)" by default.
Definition: umachine.h:156
UPRV_BLOCK_MACRO_BEGIN
#define UPRV_BLOCK_MACRO_BEGIN
Defined as the "do" keyword by default.
Definition: umachine.h:147
U16_IS_SURROGATE_LEAD
#define U16_IS_SURROGATE_LEAD(c)
Assuming c is a surrogate code point (U16_IS_SURROGATE(c)), is it a lead surrogate?
Definition: utf16.h:84
U16_GET_SUPPLEMENTARY
#define U16_GET_SUPPLEMENTARY(lead, trail)
Get a supplementary code point value (U+10000..U+10ffff) from its lead and trail surrogates.
Definition: utf16.h:112
U16_IS_SURROGATE
#define U16_IS_SURROGATE(c)
Is this code unit a surrogate (U+d800..U+dfff)?
Definition: utf16.h:75
U16_IS_TRAIL
#define U16_IS_TRAIL(c)
Is this code unit a trail surrogate (U+dc00..U+dfff)?
Definition: utf16.h:67

UTF-16: Reads the next code point (UChar32 c, out), post-increments src, and gets a value from the trie.

Sets the trie error value if c is an unpaired surrogate.

Parameters

  trie | (const UCPTrie *, in) the trie; must have type UCPTRIE_TYPE_FAST
  dataAccess | UCPTRIE_16, UCPTRIE_32, or UCPTRIE_8 according to the trie’s value width
  src | (const UChar *, in/out) the source text pointer
  limit | (const UChar *, in) the limit pointer for the text, or NULL if NUL-terminated
  c | (UChar32, out) variable for the code point
  result | (out) variable for the trie lookup result

Stable:
  ICU 63

Definition at line 386 of file ucptrie.h.

## ◆ UCPTRIE_FAST_U16_PREV

#define UCPTRIE_FAST_U16_PREV | ( |  | trie,
|  |  | dataAccess,
|  |  | start,
|  |  | src,
|  |  | c,
|  |  | result
| ) |  |

Value:
UPRV_BLOCK_MACRO_BEGIN { \
(c) = *--(src); \
int32_t __index; \
if (!U16_IS_SURROGATE(c)) { \
__index = _UCPTRIE_FAST_INDEX(trie, c); \
} else { \
uint16_t __c2; \
if (U16_IS_SURROGATE_TRAIL(c) && (src) != (start) && U16_IS_LEAD(__c2 = *((src) - 1))) { \
--(src); \
(c) = U16_GET_SUPPLEMENTARY(__c2, (c)); \
__index = _UCPTRIE_SMALL_INDEX(trie, c); \
} else { \
__index = (trie)->dataLength - UCPTRIE_ERROR_VALUE_NEG_DATA_OFFSET; \
} \
} \
(result) = dataAccess(trie, __index); \
} UPRV_BLOCK_MACRO_END
U16_IS_SURROGATE_TRAIL
#define U16_IS_SURROGATE_TRAIL(c)
Assuming c is a surrogate code point (U16_IS_SURROGATE(c)), is it a trail surrogate?
Definition: utf16.h:93
U16_IS_LEAD
#define U16_IS_LEAD(c)
Is this code unit a lead surrogate (U+d800..U+dbff)?
Definition: utf16.h:59

UTF-16: Reads the previous code point (UChar32 c, out), pre-decrements src, and gets a value from the trie.

Sets the trie error value if c is an unpaired surrogate.

Parameters

  trie | (const UCPTrie *, in) the trie; must have type UCPTRIE_TYPE_FAST
  dataAccess | UCPTRIE_16, UCPTRIE_32, or UCPTRIE_8 according to the trie’s value width
  start | (const UChar *, in) the start pointer for the text
  src | (const UChar *, in/out) the source text pointer
  c | (UChar32, out) variable for the code point
  result | (out) variable for the trie lookup result

Stable:
  ICU 63

Definition at line 417 of file ucptrie.h.

## ◆ UCPTRIE_FAST_U8_NEXT

#define UCPTRIE_FAST_U8_NEXT | ( |  | trie,
|  |  | dataAccess,
|  |  | src,
|  |  | limit,
|  |  | result
| ) |  |

Value:
UPRV_BLOCK_MACRO_BEGIN { \
int32_t __lead = (uint8_t)*(src)++; \
if (!U8_IS_SINGLE(__lead)) { \
uint8_t __t1, __t2, __t3; \
if ((src) != (limit) && \
(__lead >= 0xe0 ? \
__lead < 0xf0 ? /* U+0800..U+FFFF except surrogates */ \
U8_LEAD3_T1_BITS[__lead &= 0xf] & (1 << ((__t1 = *(src)) >> 5)) && \
++(src) != (limit) && (__t2 = *(src) - 0x80) <= 0x3f && \
(__lead = ((int32_t)(trie)->index[(__lead << 6) + (__t1 & 0x3f)]) + __t2, 1) \
: /* U+10000..U+10FFFF */ \
(__lead -= 0xf0) <= 4 && \
U8_LEAD4_T1_BITS[(__t1 = *(src)) >> 4] & (1 << __lead) && \
(__lead = (__lead << 6) | (__t1 & 0x3f), ++(src) != (limit)) && \
(__t2 = *(src) - 0x80) <= 0x3f && \
++(src) != (limit) && (__t3 = *(src) - 0x80) <= 0x3f && \
(__lead = __lead >= (trie)->shifted12HighStart ? \
(trie)->dataLength - UCPTRIE_HIGH_VALUE_NEG_DATA_OFFSET : \
ucptrie_internalSmallU8Index((trie), __lead, __t2, __t3), 1) \
: /* U+0080..U+07FF */ \
__lead >= 0xc2 && (__t1 = *(src) - 0x80) <= 0x3f && \
(__lead = (int32_t)(trie)->index[__lead & 0x1f] + __t1, 1))) { \
++(src); \
} else { \
__lead = (trie)->dataLength - UCPTRIE_ERROR_VALUE_NEG_DATA_OFFSET; /* ill-formed*/ \
} \
} \
(result) = dataAccess(trie, __lead); \
} UPRV_BLOCK_MACRO_END
U8_IS_SINGLE
#define U8_IS_SINGLE(c)
Does this code unit (byte) encode a code point by itself (US-ASCII 0..0x7f)?
Definition: utf8.h:173
U8_LEAD3_T1_BITS
#define U8_LEAD3_T1_BITS
Internal bit vector for 3-byte UTF-8 validity check, for use in U8_IS_VALID_LEAD3_AND_T1.
Definition: utf8.h:91
U8_LEAD4_T1_BITS
#define U8_LEAD4_T1_BITS
Internal bit vector for 4-byte UTF-8 validity check, for use in U8_IS_VALID_LEAD4_AND_T1.
Definition: utf8.h:108

UTF-8: Post-increments src and gets a value from the trie.

Sets the trie error value for an ill-formed byte sequence.

Unlike UCPTRIE_FAST_U16_NEXT() this UTF-8 macro does not provide the code point because it would be more work to do so and is often not needed. If the trie value differs from the error value, then the byte sequence is well-formed, and the code point can be assembled without revalidation.

Parameters

  trie | (const UCPTrie *, in) the trie; must have type UCPTRIE_TYPE_FAST
  dataAccess | UCPTRIE_16, UCPTRIE_32, or UCPTRIE_8 according to the trie’s value width
  src | (const char *, in/out) the source text pointer
  limit | (const char *, in) the limit pointer for the text (must not be NULL)
  result | (out) variable for the trie lookup result

Stable:
  ICU 63

Definition at line 451 of file ucptrie.h.

## ◆ UCPTRIE_FAST_U8_PREV

#define UCPTRIE_FAST_U8_PREV | ( |  | trie,
|  |  | dataAccess,
|  |  | start,
|  |  | src,
|  |  | result
| ) |  |

Value:
UPRV_BLOCK_MACRO_BEGIN { \
int32_t __index = (uint8_t)*--(src); \
if (!U8_IS_SINGLE(__index)) { \
__index = ucptrie_internalU8PrevIndex((trie), __index, (const uint8_t *)(start), \
(const uint8_t *)(src)); \
(src) -= __index & 7; \
__index >>= 3; \
} \
(result) = dataAccess(trie, __index); \
} UPRV_BLOCK_MACRO_END

UTF-8: Pre-decrements src and gets a value from the trie.

Sets the trie error value for an ill-formed byte sequence.

Unlike UCPTRIE_FAST_U16_PREV() this UTF-8 macro does not provide the code point because it would be more work to do so and is often not needed. If the trie value differs from the error value, then the byte sequence is well-formed, and the code point can be assembled without revalidation.

Parameters

  trie | (const UCPTrie *, in) the trie; must have type UCPTRIE_TYPE_FAST
  dataAccess | UCPTRIE_16, UCPTRIE_32, or UCPTRIE_8 according to the trie’s value width
  start | (const char *, in) the start pointer for the text
  src | (const char *, in/out) the source text pointer
  result | (out) variable for the trie lookup result

Stable:
  ICU 63

Definition at line 497 of file ucptrie.h.

## ◆ UCPTRIE_SMALL_GET

#define UCPTRIE_SMALL_GET | ( |  | trie,
|  |  | dataAccess,
|  |  | c
| ) |  | dataAccess(trie, _UCPTRIE_CP_INDEX(trie, UCPTRIE_SMALL_MAX, c))

Returns a 16-bit trie value for a code point, with range checking.

Returns the trie error value if c is not in the range U+0000..U+10FFFF.

Parameters

  trie | (const UCPTrie *, in) the trie; must have type UCPTRIE_TYPE_SMALL
  dataAccess | UCPTRIE_16, UCPTRIE_32, or UCPTRIE_8 according to the trie’s value width
  c | (UChar32, in) the input code point

Returns
  The code point's trie value.

Stable:
  ICU 63

Definition at line 370 of file ucptrie.h.

## Enumeration Type Documentation

## ◆ UCPTrieType

enum UCPTrieType

Selectors for the type of a UCPTrie.

Different trade-offs for size vs. speed.

See also
  umutablecptrie_buildImmutable
  ucptrie_openFromBinary
  ucptrie_getType

Stable:
  ICU 63

Enumerator
UCPTRIE_TYPE_ANY | For ucptrie_openFromBinary() to accept any type. ucptrie_getType() will return the actual type. Stable: ICU 63
UCPTRIE_TYPE_FAST | Fast/simple/larger BMP data structure. Use functions and "fast" macros. Stable: ICU 63
UCPTRIE_TYPE_SMALL | Small/slower BMP data structure. Use functions and "small" macros. Stable: ICU 63

Definition at line 119 of file ucptrie.h.

## ◆ UCPTrieValueWidth

enum UCPTrieValueWidth

Selectors for the number of bits in a UCPTrie data value.

See also
  umutablecptrie_buildImmutable
  ucptrie_openFromBinary
  ucptrie_getValueWidth

Stable:
  ICU 63

Enumerator
UCPTRIE_VALUE_BITS_ANY | For ucptrie_openFromBinary() to accept any data value width. ucptrie_getValueWidth() will return the actual data value width. Stable: ICU 63
UCPTRIE_VALUE_BITS_16 | The trie stores 16 bits per data value. It returns them as unsigned values 0..0xffff=65535. Stable: ICU 63
UCPTRIE_VALUE_BITS_32 | The trie stores 32 bits per data value. Stable: ICU 63
UCPTRIE_VALUE_BITS_8 | The trie stores 8 bits per data value. It returns them as unsigned values 0..0xff=255. Stable: ICU 63

Definition at line 149 of file ucptrie.h.

## Function Documentation

## ◆ ucptrie_close()

U_CAPI void ucptrie_close | ( | UCPTrie * | trie | ) |

Closes a trie and releases associated memory.

Parameters

  trie | the trie

Stable:
  ICU 63

## ◆ ucptrie_get()

U_CAPI uint32_t ucptrie_get | ( | const UCPTrie * | trie,
|  | UChar32 | c
| ) |  |

Returns the value for a code point as stored in the trie, with range checking.

Returns the trie error value if c is not in the range 0..U+10FFFF.

Easier to use than UCPTRIE_FAST_GET() and similar macros but slower. Easier to use because, unlike the macros, this function works on all UCPTrie objects, for all types and value widths.

Parameters

  trie | the trie
  c | the code point

Returns
  the trie value, or the trie error value if the code point is not in the range 0..U+10FFFF

Stable:
  ICU 63

## ◆ ucptrie_getRange()

U_CAPI UChar32 ucptrie_getRange | ( | const UCPTrie * | trie,
|  | UChar32 | start,
|  | UCPMapRangeOption | option,
|  | uint32_t | surrogateValue,
|  | UCPMapValueFilter * | filter,
|  | const void * | context,
|  | uint32_t * | pValue
| ) |  |

Returns the last code point such that all those from start to there have the same value.

Can be used to efficiently iterate over all same-value ranges in a trie. (This is normally faster than iterating over code points and get()ting each value, but much slower than a data structure that stores ranges directly.)

If the UCPMapValueFilter function pointer is not NULL, then the value to be delivered is passed through that function, and the return value is the end of the range where all values are modified to the same actual value. The value is unchanged if that function pointer is NULL.

Example:

UChar32 start = 0, end;
uint32_t value;
while ((end = ucptrie_getRange(trie, start, UCPMAP_RANGE_NORMAL, 0,
NULL, NULL, &value)) >= 0) {
// Work with the range start..end and its value.
start = end + 1;
}
UCPMAP_RANGE_NORMAL
@ UCPMAP_RANGE_NORMAL
ucpmap_getRange() enumerates all same-value ranges as stored in the map.
Definition: ucpmap.h:47
ucptrie_getRange
U_CAPI UChar32 ucptrie_getRange(const UCPTrie *trie, UChar32 start, UCPMapRangeOption option, uint32_t surrogateValue, UCPMapValueFilter *filter, const void *context, uint32_t *pValue)
Returns the last code point such that all those from start to there have the same value.
UChar32
int32_t UChar32
Define UChar32 as a type for single Unicode code points.
Definition: umachine.h:427
NULL
#define NULL
Define NULL if necessary, to nullptr for C++ and to ((void *)0) for C.
Definition: utypes.h:188

Parameters

  trie | the trie
  start | range start
  option | defines whether surrogates are treated normally, or as having the surrogateValue; usually UCPMAP_RANGE_NORMAL
  surrogateValue | value for surrogates; ignored if option==UCPMAP_RANGE_NORMAL
  filter | a pointer to a function that may modify the trie data value, or NULL if the values from the trie are to be used unmodified
  context | an opaque pointer that is passed on to the filter function
  pValue | if not NULL, receives the value that every code point start..end has; may have been modified by filter(context, trie value) if that function pointer is not NULL

Returns
  the range end code point, or -1 if start is not a valid code point

Stable:
  ICU 63

## ◆ ucptrie_getType()

U_CAPI UCPTrieType ucptrie_getType | ( | const UCPTrie * | trie | ) |

Returns the trie type.

Parameters

  trie | the trie

Returns
  the trie type

See also
  ucptrie_openFromBinary
  UCPTRIE_TYPE_ANY

Stable:
  ICU 63

## ◆ ucptrie_getValueWidth()

U_CAPI UCPTrieValueWidth ucptrie_getValueWidth | ( | const UCPTrie * | trie | ) |

Returns the number of bits in a trie data value.

Parameters

  trie | the trie

Returns
  the number of bits in a trie data value

See also
  ucptrie_openFromBinary
  UCPTRIE_VALUE_BITS_ANY

Stable:
  ICU 63

## ◆ ucptrie_openFromBinary()

U_CAPI UCPTrie* ucptrie_openFromBinary | ( | UCPTrieType | type,
|  | UCPTrieValueWidth | valueWidth,
|  | const void * | data,
|  | int32_t | length,
|  | int32_t * | pActualLength,
|  | UErrorCode * | pErrorCode
| ) |  |

Opens a trie from its binary form, stored in 32-bit-aligned memory.

Inverse of ucptrie_toBinary().

The memory must remain valid and unchanged as long as the trie is used. You must ucptrie_close() the trie once you are done using it.

Parameters

  type | selects the trie type; results in an U_INVALID_FORMAT_ERROR if it does not match the binary data; use UCPTRIE_TYPE_ANY to accept any type
  valueWidth | selects the number of bits in a data value; results in an U_INVALID_FORMAT_ERROR if it does not match the binary data; use UCPTRIE_VALUE_BITS_ANY to accept any data value width
  data | a pointer to 32-bit-aligned memory containing the binary data of a UCPTrie
  length | the number of bytes available at data; can be more than necessary
  pActualLength | receives the actual number of bytes at data taken up by the trie data; can be NULL
  pErrorCode | an in/out ICU UErrorCode

Returns
  the trie

See also
  umutablecptrie_open
  umutablecptrie_buildImmutable
  ucptrie_toBinary

Stable:
  ICU 63

## ◆ ucptrie_toBinary()

U_CAPI int32_t ucptrie_toBinary | ( | const UCPTrie * | trie,
|  | void * | data,
|  | int32_t | capacity,
|  | UErrorCode * | pErrorCode
| ) |  |

Writes a memory-mappable form of the trie into 32-bit aligned memory.

Inverse of ucptrie_openFromBinary().

Parameters

  trie | the trie
  data | a pointer to 32-bit-aligned memory to be filled with the trie data; can be NULL if capacity==0
  capacity | the number of bytes available at data, or 0 for pure preflighting
  pErrorCode | an in/out ICU UErrorCode; U_BUFFER_OVERFLOW_ERROR if the capacity is too small

Returns
  the number of bytes written or (if buffer overflow) needed for the trie

See also
  ucptrie_openFromBinary()

Stable:
  ICU 63